{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":15,"n_cols":46,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[{"$nulls":28},"A:","Ceiling to bottom of blade"]
[{"$nulls":28},"B:","Ceiling to bottom of switch housing"]
[{"$nulls":28},"C:","Ceiling to bottom of canopy"]
[{"$nulls":28},"D:","Widht of motor housing"]
[{"$nulls":28},"E:","Widht of Canopy"]
[{"$nulls":28},"F:","Ceiling to bottom of light"]
["SKU","Description","Barcode","Brand","Fan Finish","Fan Housing Material","Blade Finish","Blade Material","Diameter/Size \n(in cm)","Collapsed (cm)","Lamp","incl.","Socket","Dimmable","Summer/Winter mode","Control","Speed","Current","Blade  Pitch (Deg)","CEILING PITCH(Deg)","Motor Size (MM)","IP Rating","Poles","STANDARD DROP FROM CEILING","Wattage (Excluding Light)","Amps (h/m/l)","RPM(h/m/l)","Air flow (m3/min)","Mount system","A","B","C","D","E","F","Name and trademarks of the light bulb and each contained","N.Weight (in kg.)","G.Weight (in kg.)","Box dimensions\n(mm)","Model identifier of the lamp and / or lamp contained","Energy efficiency class of the lamp and / or lamp contained","Weighted energy consumption in kWh / 1000 hours lamp and bulb or contained","Lumen","Down rod in the package dimensions\n(mm)","Extention down rod","Remark"]
{"$rows_empty":7}
[211037,"Fanaway EVO1 LED FAN/LT W/REMOTE CH"," 9333509114529","Fanaway","chrome","Metal","Transparent","Acrylic","48\" (121cm)",47.5,"Integrated 40W LED(72pcs), 2200LM, 3 stage adjustable color temperture, 3000K, 5000K, 4000K.","yes","/","yes","yes","remote control",3,"AC","N/A",18,"D153 X 15 ","X",16,"31.5 CM",60,"0.23A/0.15A/0.1A","230/170/130",180,"Down Rod only",31.5,"N/A",10.199999999999999,47.5,15,42,null,11.8,14,"560*560*345","40W LED INCLUDED, 3000K/4000K/5000K","A",40,2200,"D26.5mm  H 127mm  1.8mm",210546]